Installing DC motor or High res stepper motor on CR model focuser



Install bracket in top hole location. Do not tighten up, let loose for now



Remove Left side knob

Remove mounting bolt

Install any require spacers at this time if clearance is needed



Tighten up bolts on non motor side

Slide motor and clutch on to shaft

Tighten up set screw on motor clutch and remove old lock knob

Once everything is in position, tighten up set screw on bracket